**CIRCUIT PIN OUT**

|  |  |  |
| --- | --- | --- |
|  | Signal pin | Power pin |
| Stepper | B7(pul),A8(dir) | N/a |
| L298N dc motor control | B12(EN),B13(IN1),B14(IN2) | N/A |
| Vibration sensor | 10 | Pwr + gnd |
| Limit switch | A11 | Pwr + gnd |
| Temperature sensor | B8, B9 |  |
| Load cell | B4, B5 |  |